**Description**

Tophammer Drilling Rig
Hours engine: approx. 1600
Hours hammer: approx. 800

Commando 120 RF is a hydraulic, self-propelled drilling unit on a 4-wheel drive carrier.
It drills holes with a maximum recommended diameter of 41 mm (1 5/8) and a maximum practical length of 9 meters (30').
Commando utilizes 19 or 22 mm (3/4 or 7/8) integral drill steels and R23 MF rods.

Specifications:

• Rock drill: HEX, hydraulic
• Engine: Caterpillar 3024C – 37 KW (50HP) / 2800 rpm
• Chain feed: CF 100 x 32 / HEX1 incl. 1 set of jaws
• Rod rack: on the carrier
• Boom: DB 120, articulated
• Carrier: Rubber-tired
• Powerpack: Diesel driven, hydraulic pumps and on-board compressor
• Hydraulic system: Open center
• Control system: TA 132E/120, radio remote
• Dust collection: DC 120, hydraulic
• Working lights: 4 pcs
• Hydraulic jacks: 4 pcs
• EU-safety devices

• Transport dimensions: 1.80 m (W) x 2.20 m (H) x 4.60 m (L)
• Weight: 2.800 kg

\_